Main.POS.Payment Service provider API ISO8583_2 ( IFSF) H2H description.NETWORK MANAGEMENT 1820/1830 - NETWORK MANAGEMENT 1820/1830

Page of - Изменено Helge Dahl в 2020/04/02 10:11

NETWORK MANAGEMENT 1820/1830

Helge Dahl

2020/04/02 10:11

Оглавление

Message authentication code (MAC) is included on network management requests to validate the MAC key issued by PayEx. PayEx recommends that this message type is the first to be implemented and tested. This will at an early stage verify that both PayEx and 3rd party has the same MAC key.

Once the integration is done and in use the network massage can be used by both the 3rd party and PayEx to monitor that the hosts can communicate, e.g there are no network issues.

NETWORK MANAGEMENT ADVICE 1820

Element number	Data element name	Presence	Format	Type	Size	Usage notes
7	Date and time, transmission	M	MMDDhhmmss	n	10	E.g.: 1025123020
11	Systems trace audit number	M	n	6	Assigned by third party host. Unique pr request
12	Date and time, local transaction	M	YYMMDDhhmmss	n	12	E.g.: 171025100515
24	Function code	M	n	3	831: System audit control / echo test. Other function codes are currently not supported.
33	Forwarding institution identification code	M	LL	n	..10	Up to 10 digit code identifying the 3rd party host. Each 3rd party integrated with PayEx will be assigned a unique code that they are to use in all messages where P-33 is specified.
53	Security Related Control Information	M	LL	b	..48	Specifies mac key version information. (53-1). See security documentation section for details.
64	MAC	M	b	8	See security documentation section for details.

NETWORK MANAGEMENT ADVICE RESPONSE 1830

Element number	Data element name	Presence	Format	Type	Size	Usage notes
7	Date and time, transmission	M	MMDDh hmmss	n	10
11	Systems trace audit number	ME	n	6
12	Date and time, local transaction	ME	YYMMD Dhhmm ss	n	12
33	Forwarding institution identification code	ME	LL	n	..11
39	Action code	M	n	3	Fixed 800 if Accepted
53	Security Related Control Information	ME	LL	b	..48
64	MAC	M	b	8